Horizontal printing density (1/inch):720
Vertical printing density (1/inch):100
Sequence length:2
Number of g values:7
Measured pitch (1/inch):40.00
Minimum g value:0
g increment:0.03
Pattern type:BOW
